# AMENDMENT No. 01

for Bid documents ICB No. № IDA/HSIP/ICB/W/2022

for procurement of works for reconstruction of the main section of heating network "Vostok" from СК-В-3а to НС№4 (I, III, IV - start-up facilities).

In accordance with clause 8 of Section I. Instructions to Bidders, OJSC “Bishkekteploset” includes and amends bid documents No. IDA/HSIP/ICB/W/2022 for procurement of works for reconstruction of the main section of heating network "Vostok" from СК-В-3а to НС№4 (I, III, IV - start-up facilities:

The following clauses and annexes are amended:

**Section IV. Bidding forms**

**Tables of Bill of Quantities for lot 1, 2 and 3**

Change the temperature 4500 C in items related to butterfly valves, ball valves, drain valves, air valves and connectors to: from 0 up to +2000 C

**Section 2 – Work requirements for the Lot 1,2 and 3**

Steel electric-welded straight-seamed heat-treated pipe of Group B made of steel St 10, GOST 1050-77, accuracy class 1, with 100% quality control of welded seams according to item 12 and bending tested according to GOST 3728-78 allowed to use steel pipes with quality not lower but higher than the requirements for steel of St 10 grade.